




























StyleView™, Black, Satin Glass

Residential Sectional Overview
Homeowners Guide to Garage Doors
Whether you are looking to enhance your home's curb appeal, add resale value, or improve garage door safety and security, Raynor Garage Doors has the residential garage door products to suit your needs.





What to Look for in a Garage Door
There are four basic types of doors for residential properties:
Pan Door (Polystyrene Insulation Optional): TradeMark™ and BuildMark®
Polystyrene Insulated Door: Encore™ EN200
Polyurethane Insulated Door: Aspen™ AP200, Aspen™ AP138, Aspen™ AP200N, Aspen™ AP200LV, Country Manor™, RockCreeke™, Eden Coast by Raynor® , and Revival Wood Collection™
Aluminum Rail and Stile Glass Doors: Raynor StyleView

With the exception of the Aluminum/Glass door, they can look very similar from the outside. So what is the correct door for your application? Why the different types?

Let's start with insulation:
Consider these two key elements:
1. What type of climate do you live in?
2. Is your garage attached? Detached? Underneath rooms (bi-level)?

Pan doors and aluminum rail and stile glass doors are not insulated. They offer virtually no thermal efficiency. Pan doors are a good choice for detached garages, or moderate climates with an attached garage. However, insulation can be added to pan doors for minimal thermal efficiency and noise suppression. Aluminum rail and stile glass doors are a great choice if aesthetics are the main concern.

Polystyrene insulated doors have three layers. Polystyrene insulation is bonded between two layers of steel providing thermal protection. These doors are a good choice for harsher climates (both cold and heat) as well as attached garages. Many aesthetic options and design elements are available to tailor these doors to your house for exceptional curb appeal.

Polyurethane insulated doors also have three layers. However, these doors feature a “foam-in-place” insulation that entirely fills all voids between the two layers of steel. Polyurethane offers the best thermal efficiency available. This is an excellent choice for attached garages, garages that are underneath rooms and harsh climates (both hot and cold). Our Aspen™ polyurethane doors also feature Raynor's proprietary WeatherLock™ section joint and seal system. As with our polystyrene doors, many aesthetic options and design elements are available.

What about windows?
Windows can add a tremendous amount of curb appeal to your door and overall appearance of your home. There are many window options available, and consider the type of door you selected to choose the correct glass. For instance, with a pan door you can choose single pane glass, but if you need an insulated door, always select insulated glass to maintain as much thermal protection as possible.

Dress it up!
Raynor has many options that can be added to increase your curb appeal. You have a choice of panel designs, color options and decorative hardware in the form of straps and handles. Don’t forget about the inside of the garage. You can upgrade from conventional galvanized hardware to EnduraCote™ hardware - a clean white powder coat system for your track and hardware and black powder coated springs and torsion tube, and add to your warranty period at the same time.

Raynor has a wide variety of doors and options to customize your garage door to your house, giving a perfect fit to your needs.
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Wind Load
Homeowners Guide to Garage Doors

Products featuring the Raynor Secure icon are available with Wind Load approved designs. See your Raynor Dealer for more details.

Raynor Recycles
Products featuring the Raynor Recycles icon are manufactured with recycled material to maintain the environment.











Creating garage doors of distinction requires the ultimate attention to detail. Raynor Distinctions Series garage doors offer the finest features the garage door industry has to offer, combined with the widest range of design options available.
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Revival Wood Collection™

Eden Coast by Raynor®

Country Manor™


		







Environmentally Friendly


· High end wood look
· Full wood overlay garage doors to achieve high end wood look
· NeuFoam™ polyurethane insulation
· WeatherLock™ section joint prevents any water from coming into your garage
· Multiple finishes and materials allow us to offer these doors in a wide assortment of traditional or contemporary designs for a custom look
· All of our windows are custom built for a one of a kind look, choose from a variety of glass options.
· Enduracote™ track, springs and hardware come standard


[image: ] Environmentally FriendlyTested U-Factor
0.17
Calculated R-Value
18.3


· High end wood look without the maintenance
· Composite full overlay garage doors to achieve high end wood look without the maintenance
· NeuFoam™ polyurethane insulation
· WeatherLock™ section joint prevents any water from coming into your garage
· Unique finishing techniques allow us to offer our doors in a wide assortment of traditional wood colors, custom designs are available
· All of our windows are custom built for a one of a kind look, choose from a variety of glass options, single pane or insulated glass is available


[image: ] Environmentally FriendlyTested U-Factor
0.17
Calculated R-Value
18.0


· Composite inlay carriage house garage door
· NeuFoam™ polyurethane insulation
· Steel, two-sided
· White, Almond, Desert Tan, Sandstone, Bronze, Brown, Slate, Black
· Arched or square window designs
· Decorative hardware options add a finishing touch.
· Features “For As Long As You Own Your Home” sections limited warranty against rust, 6-years limited warranty on hardware, and a 3-years limited warranty on springs to the original purchaser*

RockCreeke™	Raynor StyleView™

[image: ]Tested U-Factor
0.20
Calculated R-Value
13.0




Wind Load Approved

Environmentally Friendly

Wind Load Approved

Environmentally Friendly

· Composite partial overlay carriage house garage doorDistinctions Series™
* See www.raynor.com/products for complete and full Limited Warranty details.

· NeuFoam™ polyurethane insulation
· Steel, two-sided
· White, Almond, Black, Bronze, Brown, Desert Tan, Sandstone, Charcoal for Base or Board Colors
· EnduraCote™ painted track and hardware options
· Arched or square top designs
· Decorative hardware options add a finishing touch
· Optional clear, insulated and water glass available
· Features “For As Long As You Own Your Home” sections limited warranty against rust-through, trim boards for 5-years against discoloration and 10-years against delamination*
· ColorWave™: Choose from 1,500 Sherwin-Williams® colors to custom match your door to your home
· 
Aluminum rail and stile garage door
· 188 ArmorBrite™ powder coat colors available
· 3 anodized finish options available
· Elegant Finish Woodtones™
· Carriage House and Mixed Panel designs available
· 2 EnduraCote™ powder coated track and hardware options
· Alternate color kick panel options
· Dozens of glass designs to choose from including tinted, frosted, acrylic, polycarbonate and more
· Features “For As Long As You Own Your Home” section limited warranty against defects in materials and workmanship, and 5-years for ArmorBrite finish*
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Design Options
[image: ][image: ][image: ][image: ][image: ][image: ] Traditional		 Contemporary	

Window Options
[image: ]All options are available as one or two-car configurations and
square or arched top sections.	1 Pane


[image: ]	[image: ]

Bentley	Bracebridge	Style 1	Style 2	Style 3	Style 4

2 Over 2 Pane
[image: ]
3 Pane

2 Pane
[image: ]
3 Over 3 Pane



[image: ][image: ][image: ][image: ][image: ][image: ]Crosshill

Harmony

Style 5	Style 6	Style 7	Style 8



[image: ][image: ]4 Pane	4 Over 4 Pane


[image: ]	[image: ]

[image: ][image: ][image: ][image: ][image: ][image: ]Harrington	Linwood	Style 9	Style 10	Style 11	Style 12
[image: ][image: ][image: ][image: ][image: ][image: ]
Owen Sound	Oxford	Style 13	Style 14	Style 15	Style 16


Glass

5 Pane

5 Over 5 Pane






[image: ]Shakespeare



[image: ]Stratford



[image: ][image: ][image: ][image: ]Style 17	Style 18	Style 19	Style 20








Clear

Satin
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Waterloo	Windsor	Style 21	Style 22	Style 23	Style 24

Obscure

Grey Tint

Super Grey Tint


Revival Wood Collection™
Roasted
Almond
*Stain colors are shown on cedar, additional wood species and composite options are also available. Choice of overlay material will influence the door’s final appearance. The swatches shown on monitors and printed materials may vary from the actual color. For a true representation of the color, visit your local Raynor Dealer.
Revival Wood Collection, #004 Oxford Dark Oak, Bracebridge
#1108
Crimson
#005
Bedford Blue
#011
Oxford Iron Ore
#27
Onyx
#34	#004	#009
Teak	Oxford Dark	Brown
Oak	Mahogany
#3450
Special Walnut
#1134	#70
Caliwood	Walnut
#1104	#1102
Banff Brown
#1103	#17
Canyon Red	Espresso
#1101
Natural Cedar
#1105
Harvest Gold
The Revival Wood Collection is built on a durable 2” Aspen base, featuring custom wood overlays on insulated steel panels for enhanced durability and a calculated
19.25 R-Value. Available in various section heights, including 32” and 28”, each door is custom-built with your choice of finishes, combining the warmth of real wood with flexibility in design.
Stain Finishes
With both paint and stain options available, your door can be customized to match your exterior.

Many other custom options available. Contact your Raynor dealer for further details.Rain
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Eden Coast by Raynor®









Eden Coast by Raynor doors are handcrafted by fully overlaying steel sections with environmentally-friendly composite material, providing a high-end wood look without any of the maintenance.
1. Environmentally friendly, composite material
2. Square, routed, or round over edges available
3. Custom inlay molding available on square edge
4. Board thickness ranges from 1" to 1¼" to achieve desired detail
5. 2" steel sandwich door with NeuFoam™ insulation with an R-Value of 18.3
6. Doors come pre-finished in a stain color of your choice

Eden Coast by Raynor® Birmingham, Natural

Stain Finishes
Unique finishing techniques allow us to offer our doors in a variety of traditional wood colors. Finish off your authentic look by choosing an overlay in smooth or woodgrain textures.
Light Cherry	Dark Cherry
Red Mahogany
Dark Cedar
Oak
Red Walnut
Walnut
Mahogany	Driftwood
Natural

Design Options
All door designs are available in single or two-car options. Custom designs are also available!

	[image: ]
	[image: ]
	[image: ]
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	[image: ]
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	Anderson
	Asheville
	Birmingham
	Bridgemill
	Cambridge
	Charleston
	Hampton
	Leatherwood

	
[image: ]
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[image: ]
	
[image: ]
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[image: ]
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	Louisville
	Magnolia
	Magnolia-Arch
	Providence
	Saratoga
	St. Augustine
	Summerhaven
	Williamsburg



Window Options
All Eden Coast windows are custom built for a one of a kind look. Choose between clear, obscure, satin, seeded, or rain glass.
	[image: ]
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	[image: ]

	Window A
	Window B
	Window C
	Window D

	
[image: ]
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	Window E
	Window F
	Window G
	Window H

	
[image: ]
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	Window I
	Window J
	Window K
	



5










Designed to provide unsurpassed character in a maintenance-free design, Raynor RockCreeke partial overlay doors feature an environmentally stable trim board material.
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Colors
1. 
Baked-on finish
2. Epoxy primer6
3
2
1
4
5

3. Galvanized layer
4. High-strength steel
5. Polyurethane insulation
6. High-strength steel










RockCreeke, Bronze over Brown, V-Buck with 3 over 3 clear glass


Optional Track and Decorative Hardware

 Base Colors	

 Handles	

 Straps	

Standard Solid ColorsBlack



Charcoal
Board Colors
Tan
Sandstone
Brown	Desert
Bronze
White	Almond










Standard Solid ColorOptional Solid Colors
Almond	Black
Tan
Charcoal
Desert	Sandstone
Brown
Bronze
White


Optional Solid Colors


[image: ][image: ]Cast Lift Handle Fleur-de-Lis 6131100
[image: ][image: ]Cast Lift Handle Spear 6131115
[image: ][image: ]Cast Pull Handle Colonial 6131113
[image: ][image: ]Stamped Pull Handle Spade 6131102
[image: ]Low Profile Stamped Handle


Cast Pull Handle Fleur-de-Lis 6131117
Cast Pull Handle Spear 6131116
Stamped Lift Handle Spade 6131101
Stamped Bean Handles 2/pack 6130498


[image: ]
Stamped 16” Hinge
Spade (2” High)
6131105

[image: ]
Stamped 24” Hinge Spade 6131106
[image: ]
Cast 16” Hinge Spear 6131104

[image: ]
Stamped 17” Bean Straps 4/pack


[image: ]
Stamped 16” Hinge Narrow Spade (1⅝” High) 6131111

[image: ]
Cast 16” Hinge Colonial 6131114
[image: ]
Cast 16” Hinge Assembly Spear 6131103

[image: ]
Stamped 17”
Fleur-de-Lis Straps 4/pack

Fleur-de-Lis 2/pack
6130499

6130491

6130492

 Plastic Hardware Kits		 Track Options	



Optional Post Paint Finish*
Raynor’s ColorWave™ features 1,500 Sherwin-Williams® next generation post paint system options for your garage door.
*Not all colors are available in solar reflective paint, colors that are not available as solar reflective cannot be used on polyurethane doors.


[image: ]
Screw Applied Colonial Kit 4051105

Window Options*

Galvanized (standard)
[image: ]


EnduraCote™ (optional)
[image: ] [image: ]




Panel Options
Swing-Out

Bi-Fold	Accordion[image: ]
[image: ]
[image: ]
[image: ]
[image: ]
[image: ]
[image: ]
[image: ]
[image: ]
[image: ]




1 pane	1 pane arched	3 pane***

* Available in clear, water, and insulated glass
**Available in 4 over 4 pattern
3 over 3 pane**	3 over 3 pane arched** ***Available in 4 pane pattern


RockCreeke™






*Many other custom options available. Contact your Raynor dealer for further details.










With an inlay board design, this door is the ideal choice for a one of a kind carriage house look that will stand the test of time. Raynor's Country Manor is perfect balance between exceptional beauty and enduring quality. Country Manor is constructed with NeuFoam™ insulation which provides the ability to guard your garage against hot and cold temperatures; a WeatherLock™ section joint prevents air and water infiltration. Style and energy efficiency combine here to provide a comfortable climate in your garage.
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1. Baked-on finish6
3
2
1
4
5

2. Epoxy primer
3. Galvanized layer
4. High-strength steel
5. Polyurethane insulation
6. High-strength steel









Country Manor, Slate, Mission with 4-over-4-square windows.





Colors
Start creating a beautiful, customized garage door design that fits your style by selecting from one of our many color options below

Standard Solid Colors
White
Almond
Desert Tan
Sandstone



Windows
[image: ][image: ]
Square	Two Piece Arched
[image: ]
Peakview
[image: ][image: ]
4 Pane - Square	4 Pane - 2 Piece Arched


[image: ]



s




come standard with a Cool Chemistry™ pai
Black
Slate





Black steel door
Brown
Bronze




nt finish

Mission Vista



Panels

to protect from extreme heat. For environments where extreme heat and sunlight exposures are constant, black not recommended.

Wrought Iron - Square	Wrought Iron - 2 Piece
[image: ][image: ]Arched
[image: ]

[image: ][image: ][image: ]Revival Arch
[image: ] [image: ]

4-Over-4 - Square

4-Over-4 - 2 Piece Arched

[image: ]

A-Buck
Country Manor™


[image: ]
Swing

X-Buck	V-Buck
[image: ]
Mission


Glass

Spring Line









Clear	Obscure	Satin


Raynor StyleView™Clear
Dark Bronze
Black

An inspiration in both form and function, Raynor StyleView garage doors offer architectural flexibility, maximum visibility and extreme durability in a maintenance-free aluminum garage door.
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ArmorBrite™ Color System
Choose from over 188 Raynor ArmorBrite™ colors.

Anodized Finish Options
(ArmorBrite equivalents are available for shorter lead times and easier touch ups)

[image: ]
[image: ]Elegant Finish Woodtones™ Options

Aged Dark Oak

American Maple

Cherry	Cherry Flame

Colony Maple

Dark Walnut

European Cherry




Golden Oak

Knotty Pine

National Walnut

Oak	Table
Cherry

Teak

Raynor StyleView Narrow Profile


Panel Options
 Custom Carriage House	
Swing-Up


 Custom Mixed Panel	


 Narrow & Wide Profile	
Single Car
*


Swing-Out

MillCreek

MillCreek with Panels

Summitreef Summitreef
with Panels



Single car, 4'0" to 9'2", 2 panel design




[image: ]No batten


1 batten


2 batten	3 batten

Ridgelake

Bridgeport	Shoreland


Single car, 9'3" to 12'2", 3 panel design
[image: ][image: ]*


No batten	1 batten	2 batten
[image: ]Accordion


[image: ][image: ]Ridgelake with panels


[image: ]Bridgeport with panels


[image: ][image: ]Shoreland with panels




No batten	1 batten
Bi-Fold
[image: ] [image: ] [image: ]
No batten	No batten	1 batten
[image: ][image: ][image: ]
1 batten	2 batten	3 batten

Window Options
Custom Carriage House

Edgewater

[image: ]
Edgewater with panels

[image: ]
Springfield

[image: ]
Springfield with panels

Baypoint

[image: ]
Baypoint with panels

[image: ]
Brookview

[image: ]
Brookview with panels

Highcrest

[image: ]
Highcrest with panels

[image: ]
Riverside

[image: ]
Riverside with panels

[image: ] [image: ]
Double car, 12'3" to 20'0", 4 & 5 panel designs

Single-pane and two-pane options limited to 9'2" and 16'2" wide max, based on glass selection. Not all designs are available at all widths.
· Not available on narrow profile


[image: ] [image: ] [image: ] [image: ] [image: ]

[image: ][image: ][image: ][image: ]1 Pane

[image: ]
2 Pane

2 Over 2 Pane

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	


2 Over 2 Pane

3 Pane

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


3 Over 3 Pane

4 Pane

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	


4 Over 4 Pane

Prairie (Simulated Only)











Aspen Series steel garage doors provide the ultimate in safety, quality, and energy efficiency in a steel, three-layer construction door design. The Aspen Series features Raynor’s proprietary WeatherLock™ section joint and seal system, NeuFoam™ polyurethane insulation, and a multitude of panel designs.
[image: ]Aspen™ AP200LV	Aspen™ AP200N18.0
0.17
Tested U-Factor
Calculated R-Value

[image: ]		[image: ]Tested U-Factor
0.17
Calculated R-Value
18.0
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Environmentally Friendly
· Steel, two-sided
· 2” thick, NeuFoam™ polyurethane insulation
· Available in solid color or woodtone options
· Raised Colonial, Recessed Colonial Grooved, Raised Ranch, Recessed Ranch, Recessed Ranch Grooved, Flush and Plank panel designs
· Features Raynor WeatherLock™ section joint
· Optional EnduraCote™ hardware and track system
· Features “For As Long As You Own Your Home” Limited Warranty on sections and EnduraCote track and hardware, standard track and hardware 6-years and 3-years springs limited warranty*
· ColorWave™: Choose from 1,500 Sherwin-Williams® colors to custom match your door to your home
· 20% larger windows than the standard model

Environmentally Friendly
· Steel, two-sided
· 2” thick, NeuFoam™ polyurethane insulation
· Available in solid color or a woodtone option
· Flush and Plank panel designs
· Features Raynor WeatherLock™ section joint
· Optional EnduraCote™ hardware and track system
· Features “For As Long As You Own Your Home” Limited Warranty on sections and EnduraCote track and hardware, standard track and hardware 6-years and 3-years springs limited warranty*
· ColorWave™: Choose from 1,500 Sherwin-Williams® colors to custom match your door to your home
· Contemporary narrow profile windows


Aspen™ AP200	Aspen™ AP13818.0
0.17
Tested U-Factor
Calculated R-Value
13.0
0.20
Tested U-Factor
Calculated R-Value




Wind Load Approved	Environmentally Friendly
· Steel, two-sided
· 2” thick, NeuFoam™ polyurethane insulation
· Available in solid color or woodtone options
· Raised Colonial, Recessed Colonial Grooved, Raised Ranch, Recessed Ranch, Recessed Ranch Grooved, Mixed, Flush and Plank panel designs
· Features Raynor WeatherLock™ section joint
· Optional EnduraCote™ hardware and track system
· Features “For As Long As You Own Your Home” Limited Warranty on sections and EnduraCote track and hardware, standard track and hardware 6-years and 3-years springs limited warranty*
· ColorWave™: Choose from 1,500 Sherwin-Williams® colors to custom match your door to your home

Wind Load Approved	Environmentally Friendly
· Steel, two-sided
· 1-3/8” thick, NeuFoam™ polyurethane insulation
· Available in solid color or woodtone options
· Raised Colonial, Recessed Colonial Grooved, Raised Ranch, Recessed Ranch, Recessed Ranch Grooved, Mixed, Flush and Plank panel designs
· Features Raynor WeatherLock™ section joint
· Optional EnduraCote™ hardware and track system
· Features “For As Long As You Own Your Home” Limited Warranty on sections and EnduraCote track and hardware, standard track and hardware 6-years and 3-years springs limited warranty*
· ColorWave™: Choose from 1,500 Sherwin-Williams® colors to custom match your door to your home


Aspen™ Series


* See www.raynor.com/products for complete and full Limited Warranty details.

AP200LV LuxeVue™
AP200LV LuxeVue door by Raynor® combines all of the aesthetic design options of our Aspen™ Series line with a dramatically larger top window section to create a beautiful door, with stunning curb appeal.
Step out of the ordinary and compliment your home's aesthetic features with a LuxeVue™ door. The AP200LV is the perfect choice for a pristine, high-end, garage door.

Reference the LuxeVue brochure for more information on the AP200LV.
AP200LV Almond Ranch with Mission Vista Windows
Glass Options
All of our windows are tightly sealed to keep the elements out of your garage. Choose from either clear, obscure or satin glass styles.
Clear
Obscure
Satin
AP200LV Almond Ranch with Breckenridge Windows
Standard
LuxeVue™





























Window Options

	[image: ]
	[image: ]
	[image: ]
	[image: ]

	Square
	4 Pane - Square
	Wrought Iron - Square
	4-Over-4 - Square

	
[image: ]
	
[image: ]
	
[image: ]
	
[image: ]

	Two Piece Arched
	4 Pane - Two Piece Arched
	Wrought Iron - Two Piece Arched
	4-Over-4 - Two Piece Arched

	
[image: ]
	
[image: ]

	Peak View
	Spring Line

	
[image: ]
	
[image: ]

	Mission Vista
	Revival Arch
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11
system with state of the art Raynor manufacturing to craft the perfect look for their home or project.

The Aspen Contempra model is built on a 2" Aspen base and provides clean, sleek lines for the ultimate contemporary look. A low profile, and narrow frame design, make a statement while still letting natural light into the garage without sacrificing privacy.


Panel Options

	[image: ]
	[image: ]

	Flush
	Plank



Colors*
Solid Color Options
























Aspen Contempra, black with plank panels and satin glass







Glass Options
All of our windows are tightly sealed to keep the elements out of your garage. Choose from either clear, satin, or black satin glass styles.sert Tan Sandstone
Brown
Iron Ore
Slate
Black
Charcoal
Bronze
De
Almond
White




Clear	Satin	Black Satin



Aspen Elements™ Options
A collection of high-definition, digitally printed woodtone styles that embody the elemental allure of nature, blending rich grains and authentic textures to capture the essence of natural wood. Utilizing modern technology, these designs harmonize tradition with innovation, making a bold statement of style and refinement.

*Black satin available on insulated units only

Dual Aspen ElementsCocoa Hickory
Honey Cedar



[image: ]Plank Aspen ElementsCocoa Hickory
Honey Cedar



AP200N Contempra™






Optional Post Paint Finish*
Raynor’s ColorWave™ features Sherwin- Williams® next generation post paint system for your garage door. With 1,500 colors
to choose from, home and business owners can couple this elite paint










Raynor Aspen™ garage doors are available in two thickness options; 2” and 1⅜”. Both models feature NeuFoam™ insulation technology, ensuring that 100% of the section’s interior is filled with energy saving polyurethane insulation.


Aspen™ Panel Construction



1. Baked-on finish4
6
3
2
1
5

2. Epoxy primer
3. Galvanized layer
4. High-strength steel
5. Polyurethane insulation
6. High-strength steel
Aspen, black with colonial raised panel embossment and prairie windows.



*See www.raynor.com for complete and full Limited Warranty details.
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system with state of the art Raynor manufacturing to craft the perfect look for their home or project.

Colors*
Solid Color Optionssert Tan Sandstone
Brown
Iron Ore
Slate
Black
Charcoal
Bronze
De
Almond
White












Aspen Elements™ Options
A collection of high-definition, digitally printed woodtone styles that embody the elemental allure of nature, blending rich grains and authentic textures to capture the essence of natural wood. Utilizing modern technology, these designs harmonize tradition with innovation, making a bold statement of style and refinement.

Hardware Options
Standard
Aspen doors feature galvanized steel track and hinges, Egyptian coated springs, and heavy-duty nylon rollers with steel ball bearings for long life and quiet operation.

Optional
Raynor’s EnduraCote™ system includes white powder coated track, end stiles and hinges, black powder coated extended life springs and torsion bar. The EnduraCote™ option also extends the Limited Warranty* on hardware and springs to the original purchaser “For As Long As You Own Your Home” against defects in material and workmanship.

WeatherLock™ Section Joints
Aspen™ doors incorporate Raynor’s exclusive WeatherLock™ section joint. Raynor’s	proprietary	modifiedCocoa Hickory
Honey Cedar
Thermal Break - prevents heat
transfer
Air Infiltration Bulb Seal - prevents air leaks


Dual Aspen ElementsCocoa Hickory
Honey Cedar








Optional Post Paint Finish*

Plank Aspen Elements

tongue-in-groove joint provides exceptional strength, moving the joint forward to increase effectiveness of the air and water seal, keeping out unwanted water and air infiltration, while providing unyielding section strength and integrity.

Raynor’s ColorWave™ features Sherwin- Williams® next generation post paint system for your garage door. With 1,500 colors
Aspen™ AP200 & AP138

to choose from, home and business owners can couple this elite paint




Panel Options*
Aspen™ offers distinctly different panel options to help give your home a custom and unique look.
	[image: ]
	[image: ]
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	[image: ]

	Recessed Ranch
	Raised Ranch
	Recessed Ranch Grooved
	Flush

	
[image: ]
	
[image: ]
	
[image: ]
	
[image: ]

	Raised Colonial
	Recessed Colonial Grooved
	Mixed Panel
	Plank



Optional Window & Decorative Hardware*
Raynor’s many window and decorative hardware options add the finishing touches to your Aspen™ door.
These small details customize the door to your home and increase curb appeal.
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Window Options

Snap-In Inserts

	[image: ]
	[image: ]

	Clear Colonial
	Clear Ranch

	[image: ]
	
[image: ]

	Obscure Colonial
	Obscure Ranch




Decorative Hardware Options

*See Aspen Brochure for full selection.

	Handles
	
	

	Cast Lift	Cast Pull	Cast Lift	Cast Pull	Cast Pull	Stamped	Stamped	Low Profile	Low Profile Handle	Handle	Handle	Handle	Handle	Lift Handle	Pull Handle	Stamped Bean	Stamped Handle Fleur-de-Lis	Fleur-de-Lis	Spear	Spear	Colonial	Spade	Spade	Handles 2/pack	Fleur-de-Lis 2/
pack

	Straps
	
	Plastic Decorative Hardware Kits

	
[image: ]	[image: ]	[image: ]
Stamped 16” Hinge	Stamped 16” Hinge Narrow Cast 16” Hinge Colonial Spade (2” High)	Spade (1⅝” High)

[image: ]	[image: ]	[image: ]
Stamped 24” Hinge	Cast 16” Hinge Spear	Cast 16” Hinge Assembly Spade		Spear

[image: ]	[image: ]
Stamped 17” Bean Straps Stamped 17” Fleur-de-Lis 4/pack	Straps 4/pack
	
	
[image: ]	[image: ]
Screw Applied Colonial Kit  Magnetic Manor Kit

[image: ]	[image: ]
Magnetic Antique Ring Kit	Magnetic Mission Kit
*See Aspen Brochure for full selection.


[image: ]
[image: ]
Stockton Colonial
Stockton Ranch

[image: ]

[image: ]
Cascade Colonial
Cascade Ranch
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	Colonial
	
	Ranch
	
	Mixed Panel

	1-Car
	2-Car
	1-Car
	2-Car
	1-Car
	2-Car
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Glass Options
All of our windows are tightly sealed to keep the elements out of your garage. Choose from clear, obscure satin, black satin or dark tint glass styles.

Clear	Obscure	Satin

AP200 VersaView Walnut Ranch with Full View Windows
[image: ]





Black Satin*


AP200 VersaView
With Raynor's VersaView door, you have the ability to place windows in
any location on your door. Create a contemporary look with a vertical row of windows, or get creative in your window placement for a one of a kind look. The VersaView offering increases the amount of light inside your garage while improving the look of your garage door with stylish designs that enhance the curb appeal of your home! Your Raynor Dealer can build you a door with a unique look using the customizable window placement available with the VersaView program for our Aspen AP200 doors.


Dark Tint


*Black Satin available on insulated units only





[image: ]VersaView available on 2” Aspen doors only. Tempered glass must be used when placing windows in the bottom 2 sections. Max door size of 18’ 2" wide x 10’0" high. Recessed ranch panel option is not available with windows if there is an 18" section in the stack.

Encore™ - EN200 • Grey • Colonial • Stockbridge Colonial Windows










Encore Series™
Encore Series steel garage doors are beautifully designed with the homeowner in mind. These doors are strong, durable, and offer thermal benefits in a wide variety of custom design options at a competitive price.

[image: ]Encore™ EN200
[image: ]
[image: ] Wind Load Approved [image: ] Environmentally Friendly
· Steel, two-sided
· 2” thick, polystyrene insulation
· Available in 9 solid color options and a single directional woodtone option
· Colonial, Ranch, Flush, Colonial Carriage, Ranch Carriage, Plank and Shaker panel designs
· Multiple window options available
· Industry or Raynor Track and Hardware packages available
· Features “For As Long As You Own Your Home” limited warranty on section*

* See www.raynor.com/products for complete and full Limited Warranty details.
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The Raynor Encore steel two-sided residential garage door boasts both beauty and practicality. Its 2" thick sections feature a core of polystyrene insulation bonded between two high-strength, steel skins for a thermally beneficial option resulting in a 10.0 calculated R-Value*. A variety of options paired with a gunite surface texture, embossed panels and thermal benefits, give homeowners the perfect door to enhance the look of their home at an economical price point.
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Colors
Standard Solid Colors White	IvoryBrown
Taupe
Desert Tan




Optional Solid Colors
Shale	Grey	Black	Red



Optional Single Directional WoodtoneMocha*



on monitors and printed materials may vary from the actual color. For a true representation of the color, visit your local Raynor Dealer.The swatches shown

Window Options

Panel Options
Maximum opening door size*: 20’0” wide (1” increments) x 10’ high (3” increments)

	[image: ]
	[image: ]
	[image: ]

	Colonial
	Colonial Carriage
	Flush

	[image: ]
	[image: ]
	[image: ]

	Ranch
	Ranch Carriage
	Plank

	[image: ]
	
	

	Shaker
	
	




Encore™ EN200
3
*Pending testing in accordance with DASMA TDS-163
Encore, white with shaker panel embossment
2
1. High-strength steel
2. Polystyrene insulation
3. Bottom seal
1
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	Colonial
	Prairie Colonial
	Ranch
	Prairie Ranch
	Waterton Ranch
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	Waterton Colonial
	Cascade Colonial
	Cascade Ranch
	Stockbridge Ranch
	Arched Stockbridge Ranch

	
[image: ]
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	Stockbridge Colonial
	Stockton Colonial
	Stockton 10-Pane Ranch
	Stockton 8-Pane Ranch
	Arched Stockton 10-Pane Ranch

	
[image: ]
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	Berkshire 8-Pane Ranch
	
	Breckenridge
	Arched Stockton 8-Pane Ranch

	
[image: ]
	

	Berkshire 10-Pane Ranch
	













Advantage Series™
Advantage Series garage doors offer homeowners, builders, and contractors a solid pan door option with a wide-range of options and designs from which to choose.

TradeMark™	BuildMark®
[image: ]	[image: ]
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Wind Load Approved Environmentally Friendly

Wind Load Approved Environmentally Friendly

· Steel door (with optional polystyrene insulation)
· 24 gauge steel
· Available in 4 solid color options or ColorWave™
· Our beautiful window designs put the finishing touch on your garage door. Choose from clear or obscure single pane glass. Snap-in window designs add charm to any home. A variety of styles lets you customize your look!
· Features limited lifetime rust-through section warranty, 6-years track & hardware limited warranty and 3-years springs limited warranty*
· 
Steel door (with optional polystyrene insulation)
· 25 gauge steel
· Available in solid colors and ColorWave™ options
· Our beautiful window designs put the finishing touch on your garage door. Choose from clear or obscure single pane glass. Snap-in window designs add charm to any home. A variety of styles lets you customize your look!
· Features limited lifetime rust-through section warranty, 6-years track & hardware limited warranty and 3-years springs limited warranty*

TradeMark™ - White Colonial with Clear Colonial Windows


* See www.raynor.com/products for complete and full Limited Warranty details.










The combination of durable, 24-gauge steel, defined raised panel styling and authentic woodgrain texture gives your home curb appeal with TradeMark steel garage doors. Add charm with colonial or ranch panels, or for a distinctive look on your home, choose the colonial recessed grooved style. Optional polystyrene insulation can be added to provide additional comfort and help keep your garage quieter.




1. Baked-on finish
2. Epoxy primer
3. Galvanized layer
4. High-strength steel
5. Optional polystyrene insulation


TradeMark, Ranch, with Cascade Ranch inserts
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Colors
Standard Solid ColorsWhite	Almond
Standard
Bronze
Brown


Panel Options*


Colonial	Ranch



Optional Post Paint Finish*
[image: ] Raynor’s ColorWave™ features Sherwin-Williams® next generation post paint system for your garage door. With
1,500 colors to choose from, home and business owners can couple this elite paint system with state of the art Raynor manufacturing to craft the perfect look for their home or project.
*Not all colors are available in solar reflective paint, colors that are not available as solar reflective cannot be used on polyurethane doors.

Hardware Options




Colonial Recessed Grooved




Window Options
[image: ] [image: ]
Clear Colonial	Clear Ranch
[image: ][image: ]
Obscure Colonial	Obscure Ranch

Snap-In Inserts

[image: ] [image: ]	[image: ] [image: ]

[image: ]See Raynor Dealer for full hardware selection.4
2
1
3
5

TradeMark™

Hardware
TradeMark doors feature galvanized steel hardware.



Insulation Options
An energy-saving core of polystyrene insulation provides added comfort and helps keep your garage quieter.Insulated



Non-Insulated


Prairie Colonial	Prairie Ranch

[image: ] [image: ]
Stockbridge Ranch	Arched StockbridgeDecorative Hardware

Straps

[image: ]
Fleur-de-List Handle

[image: ]
Bean Handle

[image: ]




Fleur-de-Lis





[image: ]




Bean


Ranch
[image: ] [image: ]
Waterton Colonial	Waterton Ranch

[image: ] [image: ]
Cascade Colonial	Cascade Ranch

Stockton Colonial	Stockton Ranch
[image: ]
Arched Stockton Ranch
[image: ]
Berkshire
[image: ]
Breckenridge










This steel garage door design offers a traditional look at an affordable price. Choose from the time-honored ranch and colonial patterns or customize your garage with a colonial recessed grooved style. Optional polystyrene insulation can be added to provide additional comfort and help keep your garage quieter.






1. Baked-on finish
2. Epoxy primer
3. Galvanized layer
4. High-strength steel
5. Optional polystyrene insulation

BuildMark, Colonial, with Cascade Colonial inserts
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Colors
Standard Solid Colors
StandardWhite	Sandstone	Almond
Desert	Brown Tan









Optional Solid Color
Black

Hardware Options


Optional Post Paint Finish*
Raynor’s ColorWave™
features Sherwin-Williams® next generation post paint system for your garage door. With 1,500 colors to choose from, home and business owners can couple this elite paint system with state of the art Raynor manufacturing to craft the perfect look for their home or project.
*Not all colors are available in solar reflective paint, colors that are not available as solar reflective cannot be used on polyurethane doors.

Panel Options*

Colonial	Ranch

Colonial Recessed Grooved



Window Options[image: ]
[image: ]
Clear Colonial
Clear Ranch

[image: ]

[image: ]
Obscure Colonial
Obscure Ranch





[image: ][image: ]Snap-In InsertsDecorative Hardware

Straps
[image: ]
Fleur-de-List Handle

[image: ]
Bean Handle
[image: ]




Fleur-de-Lis





[image: ]




Bean

[image: ]
[image: ]
Prairie Colonial
Prairie Ranch

[image: ]

[image: ]
Stockbridge Ranch
Arched Stockbridge Ranch
[image: ]
[image: ]
Waterton Colonial
Waterton Ranch

[image: ]

[image: ]
Cascade Colonial
Cascade Ranch


Stockton Colonial	Stockton Ranch


See Raynor Dealer for full hardware selection.

Hardware
TradeMark doors feature galvanized steel hardware.



[image: ]Insulated Options
An energy-saving core of polystyrene insulation provides added comfort and helps keep your garage quieter.

Arched Stockton Ranch
[image: ]
Berkshire
[image: ]
Breckenridge

4
2
1
3
5

BuildMark®
Insulated



Non-Insulated


























Raynor offers a full line of residential openers, featuring a variety of horsepower and configuration options. All of our operators feature myQ™technology, a patented, two-way communication system that allows users to open and close the garage door and manage other household devices from anywhere in the world via a Smart Phone. Ask your authorized Raynor dealer about our residential openers, and select the ideal Raynor opener for your home.

Raynor also offers a full range of smart accessories to enhance the safety and security of your home and garage! From smart cameras that easily mount to your existing opener, to smart door locks for your main entrance, Raynor’s got you covered! With Raynor Smart Accessories you will have peace of mind from anywhere, knowing the entrances to your home are secured!




Design Center
[image: ][image: ]See what a new door can do to enhance the look of your home in real time on Raynor’s Garage Door Design Center. Select from our residential garage door models and customize your design on an uploaded image of your home or a stock photo. Visit www.designcenter.raynor.com to start designing today!Exclusively Distributed by:


Follow Us

DASMA TPV Program
[image: ]The DASMA Thermal Performance Verification (TPV) Program is a voluntary program to certify and verify the thermal performance ratings of sectional door products using third-party testing and inspection. The U-Factor on this model is verified through the DASMA TPV Program.

Residential Sectional Overview
Garage Door Openers & Smart Accessories
P.O. Box 448, 1101 East River Rd., Dixon, IL 61021-0448 1-800-4-RAYNOR (472-9667)
©2025 Raynor	2903849 1225
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